**1050铝板**具有塑性高、耐腐蚀、导电性和导热性好等特点，但强度较低。可承受各种加工压力和拉伸弯曲，气焊，氢焊和接触焊。具有较高的回收价值和良好的成型加工特性。用于PS板底座、标牌、灯具、电池软连接等。

1050 aluminum sheet & plate has the characteristics of high plasticity, corrosion resistance, good electrical and thermal conductivity, but it has lower strength. It can withstand various processing pressure, tensile bending, gas welding, hydrogen welding and contact welding. It has high recycling value and good forming processing characteristics. It is used for PS board bases, signage, lamps, battery soft connections. etc.

**应用：**

1、1050铝板可应用于锂电池软连接、化妆品瓶盖、散热片等。

2、1050铝板可用于极耳料、防爆阀、PS板基等。

Application:
1. 1050 aluminum sheet can be used in lithium battery soft connections, cosmetics bottle caps, heat sinks and so on.
2, 1050 aluminum plate can be used for tab materials, explosion-proof valves, PS plate bases, etc.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 合金ALLOY | 状态TEMPER | 厚度GAUGE | 宽度WIDTH | 长度LENGTH |
| 1050 | O, F，H12，H14、H16、H18、H19、H22、H24、H26、H28，H112,etc. | 0.1-500mm0.0039”-19.685” | 20-2650mm0.7874”-104.331” | 500-16000mm19.685”-629.921” |