**1050铝卷**具有塑性高、耐腐蚀、导电性和导热性好等特点，但强度较低。可承受各种加工压力和拉伸弯曲，气焊，氢焊和接触焊。具有较高的回收价值和良好的成型加工特性。用于PS板底座、标牌、灯具、电池软连接等。

1050 aluminum coil has the characteristics of high ductility, corrosion resistance, good electrical and thermal conductivity, but it has relatively lower strength. It can withstand various processing pressures and can be subjected to processes such as gas welding, hydrogen welding and contact welding. It has high recovery value and exhibits good formability during processing. It finds applications in PS board base, signage, lighting fixtures, battery soft connection and so on.

**应用：**

1、1050铝卷可应用于锂电池软连接、化妆品瓶盖、散热片、灯具料等。

2、1050铝卷可用于极耳料、防爆阀、PS板基、铝塑板、电容器外壳等。

Application:  
1, 1050 aluminum coil can be used in lithium battery soft connections, cosmetic bottle caps, heat sinks, lighting fixture materials, etc.  
2, 1050 aluminum coil can be used for pole lug materials, explosion-proof valves, PS plate bases, aluminum-plastic plates, capacitor shells, etc.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 合金  ALLOY | 状态  TEMPER | 厚度  GAUGE | 宽度  WIDTH | 长度  LENGTH |
| 1050 | O, F，H12，H14、H16、H18、H19、H22、H24、H26、H28，H112,etc | 0.1-8mm  0.0039”-0.315” | 400-1600mm  15.748”-62.992” | C |