**1050铝箔**密度低，导电性和导热性好，耐腐蚀性能好。1050铝箔通常是指铝含量为99.5%的铝箔。由于不需要添加其他化学元素，所以1050铝箔的生产工艺简单，价格也相对合金铝板便宜。是一种用途广泛的铝箔。

1050 aluminum foil has low density, good electrical and thermal conductivity, and good corrosion resistance.1050 aluminum foil usually refers to aluminum foil with aluminum content of 99.5%. Because it doesn't require the addition of other chemical elements, the production process of 1050 aluminum foil is simple, and its price is relatively cheaper compared to alloy aluminum sheets. It is a widely used type of aluminum foil.

应用：

1、1050铝箔可以用于食品包装、电容器、电缆带、铝箔垫片等。

Applications:
1, 1050 aluminum foil can be used in food packaging, capacitors, cable belts, aluminum foil gaskets, etc.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 合金ALLOY | 状态TEMPER | 厚度GAUGE | 宽度WIDTH | 长度LENGTH |
| 1050 | O,H14,H16,H18,H19,H22,H24 | 0.01-0.2mm0.0004”-0.0079“ | 100-1600mm3.937”-62.992” | C |