**3105铝板**具有良好的防锈性能，良好的导电性能，导电性可达41%，3105铝板在退火状态下塑性高，在半冷作硬化时塑性尚好，冷作硬化时塑性低，耐腐蚀好，焊接性良好，可切削性能不良。3105铝板属于铝锰合金，常作为装饰铝板和建材铝板使用。比如屋面铝板，瓦楞铝板，彩涂铝板等。

3105 aluminum sheet&plate has good rust resistance, good electrical conductivity, electrical conductivity up to 41%, 3105 aluminum sheet has high plasticity in the annealed state and during semi-cold hardening and has low plasticity during the cold hardening, with good corrosion resistance, good weldability, poor machinability. 3105 aluminum sheet is an aluminum-manganese alloy, often used as decorative aluminum plate and building aluminum plate. Such as roofing aluminum plate, corrugated aluminum plate, color coated aluminum plate, etc.

**应用：**

1、3105铝板常作为装饰铝板和建材铝板使用。比如屋面铝板，瓦楞铝板，彩涂铝板等。

2、3105铝板可作为房间隔断、彩涂用铝基材、灯头料、百叶窗、瓶盖、瓶塞等。

Applications:
1, 3105 aluminum plates are often used as decorative aluminum plate and building materials aluminum plate. Such as roofing aluminum plate, corrugated aluminum plate, color coated aluminum plate and so on.
2, 3105 aluminum plates can be used as room partition, color coating aluminum substrate, lamp cap material, blinds, bottle caps, bottle stoppers, etc.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 合金ALLOY | 状态TEMPER | 厚度GAUGE | 宽度WIDTH | 长度LENGTH |
| 3105 | O, F，H12，H14、H16、H18、H19、H22、H24、H26、H28，H112,etc | 0.1-500mm0.0039”-19.685” | 100-2650mm3.937”-104.331” | 500-16000mm19.685”-629.921” |