**3004铝板**是典型的Al-Mn合金，强度高于3003铝板，适用于要求强度高于3003合金的零件，具有很好的成型性，熔接性和耐蚀性。适用于灯头料，百叶窗材料，宽幅幕墙版，液晶背板料，彩涂用铝基材等。

3004 aluminum sheet & plate is a typical Al-Mn alloy, with higher strength than 3003 aluminum plate. It is suitable for parts that require higher strength than 3003 alloy, and it has good formability, weldability and corrosion resistance. It is suitable for lamp holder materials, blinds materials, wide-width curtain wall panels, liquid crystal backplate materials, aluminum substrate for color coating, etc.

**应用：**

1、3004铝板适用于灯头料、百叶窗材料、散热片、瓶盖料等。

2、3004铝板适用于宽幅幕墙版，液晶背板料，彩涂用铝基材等。

Application:

1, 3004 aluminum sheet is suitable for lamp holder materials, blinds materials, heat sinks, bottle cap materials, etc.
2, 3004 aluminum plate is suitable for wide-width curtain wall panels, liquid crystal backplate materials, aluminum substrate for color coating, etc.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 合金ALLOY | 状态TEMPER | 厚度GAUGE | 宽度WIDTH | 长度LENGTH |
| 3004 | O, F，H12，H14、H16、H18、H19、H22、H24、H26、H28，H112,etc | 0.1-500mm0.0039”-19.685” | 100-2650mm3.937”-104.331” | 500-16000mm19.685”-629.921” |