**彩涂铝带卷**的原料为纯铝或铝合金，经冷轧机轧制成不同厚度和宽度的薄铝卷。根据其用途，纵剪机将带材纵向分成不同宽度的铝带材。  
The raw material of color coated aluminum strip coil is pure aluminum or aluminum alloy, which is rolled into thin aluminum coil of different thickness and width by cold rolling machine. According to its purposes, a longitudinal slitter divides the strip into aluminum strips of different widths.

**应用：**

1、彩涂铝带卷可应用于变压器铝带(变压器铝箔)、中空玻璃铝带、散热器铝带、电缆铝带、冲压铝带等。

Applications:  
1, Color coated aluminum strip coil can be used in transformer aluminum strip (transformer aluminum foil), insulating glass aluminum strips, radiator aluminum strips, cable aluminum strips, stamping aluminum strips, etc.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 合金  ALLOY | 状态  TEMPER | 涂层厚度  COATING GAUGE | 厚度  GAUGE | 宽度  WIDTH | 长度  LENGTH |
| 1050、1060、1070、1100、3003、3004、3105、5005、5052、5754、8011 | O,H12,H14,H16,H18，H22,H24,  H26 | As per customer’s requests | 0.2-4mm  0.0079“-0.1575” | 10-200mm  0.3937“-7.874” | C |